repare file of stopflag for normal programm interruption  
read from configuration file : isEnable,isLastDest, users, passw, upfolder, arcfolder, destinationHOST, port, ~~tempfolder~~prepare temporary folders from upfolders  
\*\*\* prepare arc folders from upfolders   
\*\*\* store tempfolders files to arc  
  
  
while (continueFlag)  
 {  
  ~~\*\*\*prepare temporary folders from upfolders: folder and files if not exist or append new files if exist~~  
 }  
 for all users/destinations of conig-file do  
 {  
 check if current ip-addr is in problemIP-List do not send 10 times  
 else {  
 try send it (all the folder files), log it  
 \*\*\*remove every file was sent  
 \*\*\*remove tempfoder if is empty  
  
  
  
 on exception log it  
 add ip-addr to problemIP-List  
 }  
  
  
 ~~delete files from tempfolders~~  
 print logo  
 every 60 sec remove old files  
 wait 10 sec  
 check stopfile . if flag=1 continueFlag=false  
 read from configuration file : isEnable,isLastDest, users, passw, upfolder, ~~arcfolder,~~ destinationHOST, port

prepare temporary folders from upfolders

fill tempfolders from upfolders - change to prepare temporary folders from upfolders

fill arcfolders from upfolders  
 every 1200s check tempfolders send mail if there are many  
 }

* Config file do not contain No as upfolder  
  - sftp option  
  - may be psw encrypting  
  - tempfolders: we create temfolder for every user-destination-port on config   
   check plan :  
   1. 5 users to 3 ip  
   2. 20 users 3 not working  
   3. 20 users 3 not workig sycronized
* Q:what if tempfolder is not empty and we want to copy the same files to it?